Latch

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test scenario | D | Clk | Q | Nq |
|  | 1 | 0 | X | X |
| 1 | 1 | 1 | 1 | 0 |
| 2 | 0 | 1 | 0 | 1 |
| 3 | 0 | 0 | 0 | 1 |
| 4 | 1 | 0 | 0 | 1 |

Tff

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test scenario | T | Clk | Clear | Q |
|  | 0 | 0 | 0 | X |
| Clear asynchronously set the output to zero | 0 | 0 | 1 | 0 |
| T change to one, Output does not change | 1 | 0 | 1 | 0 |
| Clear to zero, Output does not change | 1 | 0 | 0 | 0 |
| T at one toggles output from zero to 1 on rising edge clock | 1 | 1 | 0 | 1 |
| Clear asynchronously set the output to zero clearing 1 output | 1 | 1 | 1 | 0 |
| T to zero, Output does not change | 0 | 1 | 1 | 0 |
| Clear to zero, Output does not change | 0 | 1 | 0 | 0 |
| Clock falling edge, Output does not change | 0 | 0 | 0 | 0 |
| T change to one, Output does not change | 1 | 0 | 0 | 0 |
| T at one toggles output from zero to 1 on rising edge clock | 1 | 1 | 0 | 1 |
| Clock falling edge, Output does not change | 1 | 0 | 0 | 1 |
| T at 1 toggles output from 1 to zero on rising edge clock | 1 | 1 | 0 | 0 |

Priority

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Test scenario | Sel0 | Sel1 | Sel2 | Sel4 | Z0 | Z1 | Z2 |
| Out of bounds Input set priority to 111 | 0 | 0 | 0 | 0 | 1 | 1 | 1 |
| Sel is 1000 priority is 000 | 1 | 0 | 0 | 0 | 0 | 0 | 0 |
| Sel is 0100  priority is 001 | 0 | 1 | 0 | 0 | 0 | 0 | 1 |
| Out of bounds Input set priority to 111 | 1 | 1 | 0 | 0 | 1 | 1 | 1 |
| Sel is 0010 priority is 010 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| Out of bounds Input set priority to 111 | 1 | 0 | 1 | 0 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 0 | 1 | 1 | 0 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 1 | 1 | 1 | 0 | 1 | 1 | 1 |
| Sel is 0001  Priority is 011 | 0 | 0 | 0 | 1 | 0 | 1 | 1 |
| Out of bounds Input set priority to 111 | 1 | 0 | 0 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 0 | 1 | 0 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 1 | 1 | 0 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 0 | 0 | 1 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 1 | 0 | 1 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 0 | 1 | 1 | 1 | 1 | 1 | 1 |
| Out of bounds Input set priority to 111 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |

Mux

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Test scenario | S1 | S0 | A | B | C | D | z |
| S is 00 and A (zero) is propagated to output | 0 | 0 | 0 | X | X | X | 0 |
| S is 00 and A (1) is propagated to output | 0 | 0 | 1 | X | X | X | 1 |
| S is 01 and B (zero) is propagated to output | 0 | 1 | 1 | 0 | X | X | 0 |
| S is 0 and B (1) is propagated to output | 0 | 1 | X | 1 | X | X | 1 |
| S is 10 and C (zero) is propagated to output | 1 | 0 | X | 1 | 0 | X | 0 |
| S is 10 and C (1) is propagated to output | 1 | 0 | X | X | 1 | X | 1 |
| S is 11 and D (zero) is propagated to output | 1 | 1 | X | X | 1 | 0 | 0 |
| S is 11 and D (1) is propagated to output | 1 | 1 | X | X | X | 1 | 1 |